{"text_format":"2","workbook":"xlsx","n_sheets":4,"sheets":["Menú","Códigos","Hoja1","Hoja2"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Menú","index":0,"n_rows":1,"n_cols":1,"rows_kept":1,"cut":false,"hidden":false,"merged":[[0,0,1,17]]}
["BASE DE DATOS CÓDIGOS"]

{"sheet":"Códigos","index":1,"n_rows":1048573,"n_cols":13,"rows_kept":1048573,"cut":false,"hidden":false,"merged":[]}
["EQUIPO","HP","VOLTAJE","RPM","DESCARGA","GIRO","OBSERVACIONES","FECHA","CLIENTE","NUMERO DE PEDIDO","CANTIDAD","CÓDIGO","Comentario"]
["PL-102","1/2","220/1/60",3445,null,null,"COLOCAR MOTOR 2-MO-122L","2021-01-05","BOS INTERNATIONAL",null,1,"5PL-102L"]
["CME-560","-","-","-",null,null,"AMCA TIPO C, ENHUACALADO","2021-01-05","S&P COLOMBIA",null,4,"5CME5600AMCACO"]
["CME-355","-","-","-",null,null,"AMCA TIPO C, ENHUACALADO","2021-01-05","S&P COLOMBIA",null,3,"5CME3550AMCACO"]
["CME-500","-","-","-",null,null,"AMCA TIPO C, ENHUACALADO","2021-01-05","S&P COLOMBIA",null,3,"5CME5000AMCACO"]
["CME-280","-","-","-",null,null,"AMCA TIPO C, ENHUACALADO","2021-01-05","S&P COLOMBIA",null,3,"5CME2800AMCACO"]
["CME-450","-","-","-",null,null,"AMCA TIPO C, ENHUACALADO","2021-01-05","S&P COLOMBIA",null,1,"5CME4500AMCACO"]
["CME-315","-","-","-",null,null,"AMCA TIPO C, ENHUACALADO","2021-01-05","S&P COLOMBIA",null,1,"5CME3150AMCACO"]
["CLT-28","3","230/3/60",775,null,null,"CUBREMOTOR","2021-01-05","CANAL AIR",null,1,"5CLTG28E0800CM"]
["CRVH-T-18","1 1/2","230/3/60",1550,null,null,"SW","2021-01-05","CANAL AIR",null,1,"5CRVHT18C1550S"]
["CRVL-T-12","1/4","230/3/60",1000,null,null,"SW","2021-01-05","CANAL AIR",null,1,"5CRVLT1281000S"]
["CCR-15/15","1","230/3/60",600,null,null,"SW","2021-01-05","CANAL AIR",null,1,"5CCR1515B0600S"]
["CMI-710","2","460/3/60",675,null,null,"RECUBRIMIENTO EPOXI-POLIESTER","2021-01-08","BOS INTERNATIONAL",null,1,"5CMI710D675EPX"]
["CMI-710","3","460/3/60",750,null,null,"RECUBRIMIENTO EPOXI-POLIESTER","2021-01-08","BOS INTERNATIONAL",null,1,"5CMI710E751EPX"]
["TGT/4-1250-6","40","230/3/60",1725,null,null,"ANGULO DE LA PALA \"I\"","2021-01-08","S&P COLOMBIA",null,4,"5TGT4125064ICO"]
["TGT/4-1250-3","30","230/3/60",1725,null,null,"ANGULO DE LA PALA \"L\"","2021-01-08","S&P COLOMBIA",null,1,"5TGT4125033LCO"]
["IFHT-100/4/8-NC","2.5/0.45 KW","460/3/60","1730 / 875",null,null,"CON CAJA DE BORNES","2021-01-12","S&P COLOMBIA",null,1,"5IFHT-100NCO"]
["IFHT-50/4/8-NC","1.5/0.21 KW","460/3/60","1690 / 885",null,null,"CON CAJA DE BORNES","2021-01-12","S&P COLOMBIA",null,1,"5IFHT-501NCO"]
["CCR-12/12","1/2","230/3/60",650,null,null,null,"2021-01-12","VENTILACION INDUSTRIAL",null,1,"5CCR1212906500"]
["IWXT-800-1/2","1/2","230/3/60",530,null,null,"BRIIDAS EN DESCARGA Y SUCCION","2021-01-13","BV EQUIPOS INDUSTRIAL",null,2,"FORMATO"]
["CLT-18","3","230/3/60",1250,null,null,"COLOCAR MOTOR  2-MO-067XUS, CUBREMOTOR","2021-01-19","S&P PERÚ",null,2,"5CLTG18E125APX"]
["CCK-9/9","1/2","220/1/60",1000,null,null,null,"2021-01-21","REFRIMUNDO",null,2,"5CCK9940100000"]
["CRVLT-26","-","-","-",null,null,"EJE MILIMETRICO  28 MM","2021-01-22","S&P Chile",null,3,"5CRVLT260000CL"]
["CLT-7","-","-","-",null,null,"DESARMADO","2021-01-29","S&P PERÚ",null,2,"5CLTL-77PU"]
["HGT-1500-3","-","-","-",null,null,"DESARMADO, SIN MOTOR, CON TRANSMISION","2021-01-29","S&P PERÚ",null,10,"5HGT15003PU"]
["WALL COLLAR-800","-","-","-",null,null,"CAJON WALL COLLAR TAMAÑO 800","2021-01-29","REFRIMUNDO",null,4,"5ZCA800WC","Existe"]
["TGT/6-1000-9/3","3","230/3/60",1150,null,null,"ANGULO DE LA PALA C","2021-02-03","S&P COLOMBIA",null,1,"5TGT6100093CCO"]
["CLTL-14","-","-","-",null,null,"DESARMADO","2021-02-04","S&P PERÚ",null,2,"5CLT-014PU"]
["CRVLT-16","3/4","230/3/60",1000,null,null,null,"2021-02-10","SOLUCIONES EN FRIO",null,1,"5CRVLT16A01000"]
["HGT-1500-3","-","-","-",null,null,"DESARMADO, SIN MOTOR, CON TRANSMISION, PINTURA EPOXICA","2021-02-15","S&P PERÚ",null,20,"5HGT15003XPU"]
["CLTL-12","1","220/1/60",1817,null,null,"CUBREMOTOR","2021-03-03","SERKING",null,1,"5CLTG1261817CM"]
["CLTL-16","1 1/2","220/1/60",1350,null,null,"CUBREMOTOR","2021-03-03","SERKING",null,1,"5CLTG1671350CM"]
["IFHT-50/4/8-NC","1.5/0.21 KW","230/3/60","1690 / 885",null,null,"CON CAJA DE BORNES","2021-03-17","S&P COLOMBIA",null,30,"5IFHT-502NCO"]
["UMF-250","-","-","-",null,null,"OCUPAR ESTA ESTRUCTURA 5UMF-250CL Y AGREGAR MOTOR 2-RE-192EC","2021-03-18","S&P CHILE",null,50,"5UMF-251CL"]
["TGT/4-1000-3/7.5","7 1/2","230/3/60",1725,null,null,"PIE SOPORTE ANGULO DE  LA PALA H","2021-03-23","MOEGSA",null,8,"5TGT4100037PSH"]
["TGT/4-1000-3/7.5","7 1/2","230/3/60",1725,null,null,"PIE SOPORTE ANGULO DE  LA PALA G","2021-03-23","MOEGSA",null,8,"5TGT4100037PSG"]
["HXP/8-1000/H","1","230/3/60",865,null,null,"WALL COLLAR, MALLA EN SUCCION, SW","2021-03-25","S&P COLOMBIA",null,1,"5HXP8-1000HMCO"]
["CRVLT-16","1 1/2","220/1/60",1100,null,null,null,"2021-03-29","ALASKA COOL",null,1,"5CRVLT16701100"]
["CCR-12/12","1 1/2","220/1/60",600,null,null,null,"2021-03-29","ALASKA COOL",null,1,"5CCR1212706000"]
["HXP/8-1000/H","1","230/3/60",865,null,null,"WALL HOUSING, MALLA EN SUCCION, MALLA EN DESCARGA, SW","31/09/2021","S&P COLOMBIA",null,1,"5HXP8-1001HMCO"]
["CLT-12","1/2","220/1/60",1600,null,null,"ACTIVAR CÓDIGO 5CLTG1241600CM","2021-04-07","COPPER GROUP",null,1,"5CLTG1241600CM"]
["HEP-400","1/4","230/1/60",1750,null,null,"MOTOR  2-MO-140MRX","2021-04-16","S&P PERÚ",null,1,"CANCELADO"]
["HGT-1000-3/4","3/4","230/3/60",550,null,null,"RECUBRIMIENTO EPOXI-POLIESTER","2021-04-23","S&P COLOMBIA",null,2,"5HGT1000LEPXCO"]
["IWXT-800-1/2","1/2","230/3/60",530,null,null,"BANCO PORTAFILTROS, PERSIANA DE INYECCION, MALLA EN LA DESCARGA ","2021-04-28","BV EQUIPOS INDUSTRIAL",null,6,"FORMATO"]
["CDAHF1-20/20","1 1/2","230/3/60",400,null,null,null,"2021-04-28","BV EQUIPOS INDUSTRIAL",null,1,"5CDAHF120C0400"]
["CDAHF2-22/22","10","230/3/60",650,null,null,null,"2021-04-29","BOS INTERNATIONAL",null,1,"5CDAHF222H0650"]
["CRVL-T-18","1/2","230/3/60",1150,null,null,"TRAMPA GRASERA","2021-04-30","BV EQUIPOS INDUSTRIAL",null,2,"5CRVLT189115TG"]
["CMI-1400","40","230/3/60","600",null,null,null,"2021-05-04","BV EQUIPOS INDUSTRIAL",null,3,"5CMI1400R06000"]
["HGB-1000-1","1","220/1/60","610",null,null,"COLOCAR MOTOR 2-MO-140MR","2021-05-05","BOS INTERNATIONAL",null,1,"5HGB1000L1610"]
["CLT-16","-","-","-",null,null,"DESARMADO","2021-05-13","S&P PERÚ",null,1,"5CLT-16/16DES"]
["CMI-900","3","460/3/60","525",null,null,"SW, MALLA EN SUCCION, ,MALLA EN DESCARGA","2021-05-17","BOS INTERNATIONAL",null,2,"5CMI900E0525MA"]
["CCK-18/18","5","460/3/60","750",null,null,"SW","2021-05-17","BOS INTERNATIONAL",null,1,"5CCK1818F0750S"]
["CLTH-16","5","230/3/60","1900",null,null,"SW, CUBREMOTOR","2021-05-19","EURO-AIRE",null,1,"5CLTH16F1900CM"]
["CLTL-16","2","230/3/60","1500",null,null,"SW, CUBREMOTOR","2021-05-19","EURO-AIRE",null,1,"5CLTG16D1500CM"]
["CRVL-T-18","1 1/2","230/3/60",1200,null,null,"TRAMPA GRASERA","2021-05-19","EURO-AIRE",null,1,"5CRVLT18C120TG"]
["CRVL-T-14","1/2","230/3/60",1650,null,null,"TRAMPA GRASERA","2021-05-19","EURO-AIRE",null,1,"5CRVLT149165TG"]
["CRVL-T-16","1 1/2","230/3/60",1300,null,null,"TRAMPA GRASERA","2021-05-19","EURO-AIRE",null,1,"5CRVLT16C130TG"]
["CRVL-T-18","1 1/2","230/3/60",1325,null,null,"TRAMPA GRASERA","2021-05-19","EURO-AIRE",null,1,"5CRVLT18C132TG"]
["CRVH-T-14","1","220/1/60",2000,null,null,"TRAMPA GRASERA","2021-05-19","EURO-AIRE",null,1,"5CRVHT146200TG"]
["CRVL-T-20","2","220/1/60",1275,null,null,"TRAMPA GRASERA","2021-05-19","EURO-AIRE",null,1,"5CRVLT201127TG"]
["CRVL-T-16","1","220/1/60",1150,null,null,"TRAMPA GRASERA","2021-05-19","EURO-AIRE",null,1,"5CRVLT166115TG"]
["CRVL-T-10","1/4","220/1/60",1325,null,null,"TRAMPA GRASERA","2021-05-19","EURO-AIRE",null,1,"5CRVLT102132TG"]
["CLTH-10","3/4","220/1/60",2000,null,null,"CUBREMOTOR","2021-05-19","EURO-AIRE",null,3,"5CLTH1052000CM"]
["CLTH-10","3/4","220/1/60",1850,null,null,"CUBREMOTOR","2021-05-19","EURO-AIRE",null,1,"5CLTH1051850CM"]
["CCR-18/18","1 1/2","220/1/60",675,null,null,null,"2021-05-19","EURO-AIRE",null,1,"5CCR1818767500"]
["CLT-10","1/2","220/1/60",1725,null,null,"CUBREMOTOR","2021-05-19","EURO-AIRE",null,1,"5CLTG1041725CM"]
["DXT-1000/L-3/4T","3/4","230/3/60",700,null,null,null,"2021-05-21","BV EQUIPOS INDUSTRIAL",null,4,"5DX100034S"]
["CRVH-T-18","3","208/3/60",1600,null,null,"TRAMPA GRASERA, COLOCAR EL MOTOR 2-MO-342MR","2021-05-19","EURO-AIRE",null,1,"5CRVHT18E160TG"]
["KITREFACCIONES CLT7",{"$nulls":5},"COLOCAR CÓDIGOS 3-CH-07GN, 3-EM-07GN, 3-ZTB-7","2021-06-11","S&P COLOMBIA",null,1,"5KIT CLT-07CO"]
["KITREFACCIONES CLT10",{"$nulls":5},"COLOCAR CÓDIGOS 3-CH-010N, 3-EM-010GN, 3-ZTB-010","2021-06-11","S&P COLOMBIA",null,1,"5KIT CLT-10CO"]
["KITREFACCIONES CLT14",{"$nulls":5},"COLOCAR CÓDIGOS 3-CH-14G, 3-EM-14GL, 3-ZTB-014","2021-06-11","S&P COLOMBIA",null,1,"5KIT CLT-14CO"]
["KITREFACCIONES CLT16",{"$nulls":5},"COLOCAR CÓDIGOS 3-CH-16G, 3-EM-16GL, 3-ZTB-016","2021-06-11","S&P COLOMBIA",null,1,"5KIT CLT-16CO"]
["KITREFACCIONES CLT18",{"$nulls":5},"COLOCAR CÓDIGOS 3-CH-18N, 3-EM-18GN, 3-ZTB-018","2021-06-11","S&P COLOMBIA",null,1,"5KIT CLT-18CO"]
["KITREFACCIONES CLT20",{"$nulls":5},"COLOCAR CÓDIGOS 3-CH-20N, 3-EM-20GN, 3-ZTB-020","2021-06-11","S&P COLOMBIA",null,1,"5KIT CLT-20CO"]
["KITREFACCIONES CLT24",{"$nulls":5},"COLOCAR CÓDIGOS 3-CH-24N, 3-EM-24N, 3-ZTB-088","2021-06-11","S&P COLOMBIA",null,1,"5KIT CLT-24CO"]
["KITREFACCIONES CLT26",{"$nulls":5},"COLOCAR CÓDIGOS 3-CH-26GN, 3-EM-26GN, 3-ZTB-089","2021-06-11","S&P COLOMBIA",null,1,"5KIT CLT-26CO"]
["KITREFACCIONES CLT28",{"$nulls":5},"COLOCAR CÓDIGOS 3-CH-28GN, 3-EM-28GN, 3-ZTB-090","2021-06-11","S&P COLOMBIA",null,1,"5KIT CLT-28CO"]
["CRVLT-16","3/4","220/1/60",1300,null,null,"TRAMPA GRASERA","2021-06-15","AIRE FRIO DE HONDURAS",null,2,"5CRVLT165131TG"]
["CRVLT-18","1","220/1/60",1200,null,null,"TRAMPA GRASERA","2021-06-15","AIRE FRIO DE HONDURAS",null,6,"5CRVLT186120TG"]
["CRVLT-20","1 1/2","127/1/60",1230,null,null,"TRAMPA GRASERA","2021-06-15","AIRE FRIO DE HONDURAS",null,14,"5CRVLT207123TG"]
["CRVLT-24","1 1/2","127/1/60",800,null,null,"TRAMPA GRASERA","2021-06-15","AIRE FRIO DE HONDURAS",null,6,"5CRVLT247800TG"]
["TBN-T-I-630","15","230/3/60",1700,null,null,null,"2021-06-16","MOEGSA",null,1,"5TBNTI630M1700"]
["CLT-16","2","230/3/60",1500,null,null,"CUBREMOTOR","2021-06-16","MOEGSA",null,2,"5CLTG16D1501CM"]
["CLT-16","1 1/2","230/3/60",1400,null,null,"CUBREMOTOR","2021-06-16","MOEGSA",null,2,"5CLTG16C1400CM"]
["CRHLT-10","1/4","230/3/60",1125,null,null,null,"2021-06-16","REFRICENTRO",null,2,"5CRHLT10801125"]
["CDAVF2-30/28","10","460/3/60",375,null,null,null,"2021-06-28","BOS INTERNATIONAL",null,4,"5CDAVF2328H375"]
["CRVHT-33","10","460/3/60",800,null,null,"MOTOR USO VARIADOR  (2-MO-083US)","2021-07-05","S&P COLOMBIA",null,2,"5CRVHT33H800CO"]
["CRVLT-12","1/4","460/3/60",850,null,null,null,"2021-07-05","S&P COLOMBIA",null,2,"5CRVLT128850CO"]
["C/DAHF2-18/18","5","460/3/60",750,null,null,"MOTOR USO VARIADOR (2-MO-6518), FILTROS LAVABLES METALICOS PRIMERA ETAPA, FILTROS PLISADOS MERV 8  SEGUNDA ETAPA , PINTURA POLIESTER","2021-07-05","S&P COLOMBIA",null,2,"5CDAHF218F75CO"]
["CDAH-15/15","3","460/3/60",725,null,null,"MOTOR USO VARIADOR (2-MO-347MR), PINTURA POLIESTER","2021-07-05","S&P COLOMBIA",null,2,"5CDAH1515E72CO"]
["CRVHT-33","5","460/3/60",675,null,null,"MOTOR USO VARIADOR (2-MO-542US) ","2021-07-05","S&P COLOMBIA",null,10,"5CRVHT33F675CO"]
["CDAH-12/12","3/4","460/3/60",725,null,null,"MOTOR USO VARIADOR (2-MO-034US) PINTURA POLIESTER","2021-07-05","S&P COLOMBIA",null,2,"5CDAH1212A72CO"]
["DXD-1000-1HP-8P-A","1","460/3/60",865,null,null,"MALLA DE PROTECCION EN ASPIRACION, MALLA DE PROTECCION EN DESCARGA, RECUBRIMIENTO POLIESTER, MOTOR USO VARIADOR(2-MO-018MR)","2021-07-12","S&P COLOMBIA",null,3,"5DXD10001886CO"]
["DXD-1000-1.5 HP- 6P-A","1 1/2","460/3/60",1165,null,null,"MALLA DE PROTECCION EN ASPIRACION, MALLA DE PROTECCION EN DESCARGA, RECUBRIMIENTO POLIESTER, MOTOR USO VARIADOR (2-MO-166MR)","2021-07-12","S&P COLOMBIA",null,1,"5DXD10001126CO"]
["DXD-1000-2 HP 6P-A","2","460/3/60",1165,null,null,"MALLA DE PROTECCION EN ASPIRACION, MALLA DE PROTECCION EN DESCARGA, RECUBRIMIENTO POLIESTER, MOTOR USO VARIADOR (2-MO-126MR)","2021-07-12","S&P COLOMBIA",null,2,"5DXD10002611CO"]
["DXT-1500-3TF","3","460/3/60","550",null,null,"MALLA DE PROTECCION EN ASPIRACION, MALLA DE PROTECCION EN DESCARGA, RECUBRIMIENTO POLIESTER, MOTOR USO VARIADOR(2-MO-347MR)","2021-07-12","S&P COLOMBIA",null,7,"5DXT15003550CO"]
["DXT-1500-5TF","5","460/3/60","550",null,null,"MALLA DE PROTECCION EN ASPIRACION, MALLA DE PROTECCION EN DESCARGA, RECUBRIMIENTO POLIESTER, MOTOR USO VARIADOR (2-MO-6518)","2021-07-12","S&P COLOMBIA",null,4,"5DXT15005550CO"]
["DXT-800/L","1/2","460/3/60",530,null,null,"MALLA DE PROTECCION EN ASPIRACION, MALLA DE PROTECCION EN DESCARGA, RECUBRIMIENTO POLIESTER, MOTOR USO VARIADOR (2-MO-124MR)","2021-07-12","S&P COLOMBIA",null,3,"5DXT80012530CO"]
["HAB/6-500/H","1/2","460/3/60",1150,null,null,"MOTOR USO VARIADOR (2-MO-074MT)","2021-07-12","S&P COLOMBIA",null,1,"5HAB6-500/28CO"]
["HAT/4-400/H","1/4","460/3/60",1725,null,null,"MOTOR USO VARIDOR (2-MO-025MR)","2021-07-12","S&P COLOMBIA",null,2,"FORMATO"]
["HEP-500","1/2","460/3/60",1740,null,null,"PERSIANA DE EXTRACCION, WALL HOUSING(RECUBRIMIENTO POLIESTER) ","2021-07-12","S&P COLOMBIA",null,2,"5HEP-500CO"]
["IDXD-1000-2-A","2","460/3/60",1165,null,null,"FILTROS PLISADOS MERV 10, RECUBRIMIENTO POLIESTER, MALLA DE PROTECCION EN DESCARGA, MOTOR USO VARIADOR(2-MO-126MR)","2021-07-12","S&P COLOMBIA",null,1,"5IDXD1000211CO"]
["IDXD-800-1T 6P-A","1","460/3/60",1165,null,null,"FILTROS PLISADOS MERV 10, RECUBRIMIENTO POLIESTER, MALLA DE PROTECCION EN DESCARGA, MOTOR USO VARIADOR (2-MO-116MR)","2021-07-12","S&P COLOMBIA",null,3,"5IDXD8001611CO"]
["IDXT-1500-10","10","460/3/60",550,null,null,"FILTROS PLISADOS MERV 10, RECUBRIMIENTO POLIESTER, MALLA DE PROTECCION EN DESCARGA MOTOR USO VARIADOR (2-MO-083US)","2021-07-12","S&P COLOMBIA",null,4,"5IDXT1500H55CO"]
["IDXT-1500-3","3","460/3/60",550,null,null,"FILTROS PLISADOS MERV 10, RECUBRIMIENTO POLIESTER, MALLA DE PROTECCION EN DESCARGA, MOTOR USO VARIADOR(2-MO-347MR)","2021-07-12","S&P COLOMBIA",null,2,"5IDXT1500355CO"]
["IDXT-1500-5","5","460/3/60",550,null,null,"FILTROS PLISADOS MERV 10, RECUBRIMIENTO POLIESTER, MALLA DE PROTECCION EN DESCARGA, MOTOR USO VARIADOR (2-MO-6518)","2021-07-12","S&P COLOMBIA",null,7,"5IDXT1500555CO"]
["IDXT-800/L","1/2","460/3/60",530,null,null,"FILTROS PLISADOS MERV 10, RECUBRIMIENTO POLIESTER, MALLA DE PROTECCION EN DESCARGA, MOTOR USO VARIADOR (2-MO-124MR)","2021-07-12","S&P COLOMBIA",null,4,"5IDXT8001253CO"]
["IDXT-800/L1","3/4","460/3/60",700,null,null,"FILTROS PLISADOS MERV 10, RECUBRIMIENTO POLIESTER, MALLA DE PROTECCION EN DESCARGA, MOTOR USO VARIADOR (2-MO-034US)","2021-07-12","S&P COLOMBIA",null,2,"5IDXT8003470CO"]
["IWXD-630-3/4","3/4","460/3/60",1130,null,null,"PERSIANA DE INYECCION, RECUBRIMIENTO POLIESTER, BANCO PORTAFILTROS BRIDADO, FILTROS PLISADOS MERV-10,CAJA BRIDADA, MALLA EN DESCARGA  MOTOR USO VARIADOR (2-MO-356MR).","2021-07-12","S&P COLOMBIA",null,2,"FORMATO"]
["IWXD-630-3/4","3/4","460/3/60",1130,null,null,"PERSIANA DE INYECCION, RECUBRIMIENTO POLIESTER, BANCO PORTAFILTROS BRIDADO, FILTROS PLISADOS MERV-7,CAJA BRIDADA, MALLA EN DESCARGA  MOTOR USO VARIADOR (2-MO-356MR).","2021-07-12","S&P COLOMBIA",null,6,"FORMATO"]
["AGIT-1250",{"$nulls":5},"SIN MOTOR, Y SIN POLEA MOTRIZ SIN BANDA","2021-07-13","S&P Chile ",null,4]
["CMI-250","3/4","460/3/60",2575,null,null,null,"2021-07-21","VENTILACION INDUSTRIAL",null,1,"5CMI250A025750"]
["CDAHF2-9/9","3/4","460/3/60",1225,null,null,null,"2021-07-21","VENTILACION INDUSTRIAL",null,1,"5CDAHF299A1225"]
["CMII-355",{"$nulls":5},"ENHUACALADO","2021-07-21","S&P COLOMBIA",null,1,"5CMII3550000CO"]
["CMII-450",{"$nulls":5},"ENHUACALADO","2021-07-21","S&P COLOMBIA",null,1,"5CMII4500000CO"]
["CMII-500",{"$nulls":5},"ENHUACALADO","2021-07-21","S&P COLOMBIA",null,1,"5CMII5000000CO"]
["CMII-630","-","-","-","TH","CCW","ENHUACALADO","2021-07-28","S&P COLOMBIA",null,1,"5CMII630000ICO"]
["CCK-10/10","3/4","127/1/60",800,null,null,"ENHUCALADO","2021-08-09","REFRIMUNDO",null,1,"5CCK1010508001"]
["CRWL-T-16","1/2","220/1/60",1000,null,null,"COLOCAR MOTOR (2-MO-120MRX)","2021-08-10","BOS INTERNATIONAL",null,1,"5CRWLT16401000"]
["C/DAVF2-12/12","1","220/1/60",1025,null,null,"FILTROS LAVABLES METALICOS PRIMERA ETAPA, FILTROS PLISADOS MERV-13 SEGUNDA ETAPA, ENHUACALADO","2021-08-10","BOS INTERNATIONAL",null,1,"5CDAVF21261025"]
["BDBI-1000","-","-","-",null,null,"SIN MOTOR, NI TRANSMISION, DESARMADO","2021-08-13","S&P COLOMBIA",null,4,"5BDBI1000000CO"]
["HGTA-1000/H","3/4","230/3/60",475,null,null,null,"2021-08-13","BV EQUIPOS INDUSTRIAL",null,1,"5HGTA1000HA475"]
["CRVH-T-24","3","230/3/60",1025,null,null,"SW,TRAMPA DE GRASA","2021-08-17","REFRIMUNDO",null,1,"5CRVHT24E102TG"]
["CRHL-T-14","1/2","220/1/60",1575,null,null,"SW","2021-08-17","REFRIMUNDO",null,1,"5CRHLT1441575S"]
["CDAVF1-18/18","2","230/3/60",700,null,null,"SW","2021-08-17","REFRIMUNDO",null,1,"5CDAVF118D700S"]
["RBC-630","3/4","230/3/60",1135,null,null,"COLOCAR MOTOR 2-MO-356MR","2021-08-18","S&P COLOMBIA",null,4,"5RBC630CO"]
["RBC-800","1","230/3/60",1150,null,null,"COLOCAR MOTOR 2-MO-116MR","2021-08-18","S&P COLOMBIA",null,8,"5RBC800CO"]
["CLT-22","2","220/1/60",975,null,null,null,"2021-08-20","REFRIMUNDO",null,1,"5CLTG221097500"]
["CMI-500","3","230/3/60",1525,null,null,"DISCO DE ENFRIAMIENTO, SELLO EN FLECHA, RECUBRIMIENTO ALTAS TEMPERATURAS","2021-08-23","MOEGSA",null,1,"5CMI500E1525AT"]
["CLT-36","2","230/3/60",475,null,null,"CUBREMOTOR","2021-08-23","SOLUCIONES EN FRIO",null,2,"5CLTG36D0475CM"]
["TGT/4-1000-3/10","10","230/3/60",1725,null,null,"ANGULO DE LA PALA I, PIES SOPORTES","2021-08-24","CFM TECNOLOGIES",null,1,"5TGT4100031IPS"]
["IWXD-630-3/4","3/4","460/3/60",1130,null,null,"PERSIANA DE INYECCION, RECUBRIMIENTO POLIESTER, BANCO PORTAFILTROS BRIDADO, FILTROS PLISADOS MERV-10,CAJA BRIDADA, MALLA EN DESCARGA  SIN MOTOR","2021-08-25","S&P COLOMBIA",null,2,"FORMATO"]
["DXD-1000-1.5 HP- 6P-A","1 1/2","460/3/60",1165,null,null,"MALLA DE PROTECCION EN ASPIRACION, MALLA DE PROTECCION EN DESCARGA, RECUBRIMIENTO POLIESTER, SIN MOTOR ","2021-08-25","S&P COLOMBIA",null,1,"5DXD1000SMCO"]
["IWXD-630-3/4","3/4","460/3/60",1130,null,null,"PERSIANA DE INYECCION, RECUBRIMIENTO POLIESTER, BANCO PORTAFILTROS BRIDADO, FILTROS PLISADOS MERV-7,CAJA BRIDADA, MALLA EN DESCARGA , SIN MOTOR","2021-08-25","S&P COLOMBIA",null,6,"FORMATO"]
["IWXD-630-3/4","3/4","460/3/60",1130,null,null,"PERSIANA DE INYECCION, RECUBRIMIENTO POLIESTER, BANCO PORTAFILTROS BRIDADO, FILTROS PLISADOS MERV-10,CAJA BRIDADA, MALLA EN DESCARGA ","2021-08-25","S&P COLOMBIA",null,2,"FORMATO"]
["KITREFACCIONES CLTH10","-","-","-",null,null,"COLOCAR CÓDIGOS 3-CH-010N, 3-EM-010GN, 3-ZTB-102N","2021-08-25","S&P COLOMBIA",null,1,"5KIT CLTH-10CO"]
["KITREFACCIONES CLTH14","-","-","-",null,null,"COLOCAR CÓDIGOS 3-CH-14G, 3-EM-14GL, 3-ZTB-142","2021-08-25","S&P COLOMBIA",null,1,"5KIT CLTH-14CO"]
["KITREFACCIONES CLTH16","-","-","-",null,null,"COLOCAR CÓDIGOS 3-CH-16G, 3-EM-16GL, 3-ZTB-162","2021-08-25","S&P COLOMBIA",null,1,"5KIT CLTH-16CO"]
["KITREFACCIONES CLTH18","-","-","-",null,null,"COLOCAR CÓDIGOS 3-CH-18N, 3-EM-18GN, 3-ZTB-182","2021-08-25","S&P COLOMBIA",null,1,"5KIT CLTH-18CO"]
["KITREFACCIONES CLTH20","-","-","-",null,null,"COLOCAR CÓDIGOS 3-CH-20N, 3-EM-20GN, 3-ZTB-202","2021-08-25","S&P COLOMBIA",null,1,"5KIT CLTH-20CO"]
["KITREFACCIONES CLTH12","-","-","-",null,null,"COLOCAR CÓDIGOS 3-CH-12N, 3-EM-12GN, 3-ZTB-012N","2021-08-25","S&P COLOMBIA",null,1,"5KIT CLTH-12CO"]
["WXD-630-1/2-6P/L","1/2","230/3/60","1150",null,null,null,"2021-08-01","REFRIMUNDO",null,1,"5WXD63091150"]
["IFFT-100N230I","0.45 KW","230/3/60","875",null,null,"SIN INTERRUPTOR","2021-09-01","S&P COLOMBIA",null,4,"5IFFT-100N23CO"]
["CCL-9/9","3/4","220/1/60",1200,null,null,null,"03/09/201","REFRIMUNDO",null,1,"5CCL9950120000"]
["KITREFACCIONES CLT33","-","-","-",null,null,"3-CH-33GN, 3-ZTB-332A, 3-EM-33GN","2021-09-08","S&P COLOMBIA",null,4,"5KIT CLT-33CO"]
["CMII1000","-","-","-",null,null,"EJE MILIMETRICO  63 MM (La informacion del Dibujo se manejara mediante correos)","2021-09-08","S&P CHILE",null,1,"5CMII1000000CL"]
["CRVLT-24","1","230/3/60",675,null,null,null,"2021-09-20","BOS INTERNATIONAL",null,2,"5CRVLT24B06750"]
["CDAHF2-18/18","3","460/3/60",825,null,null,"SWITCH, FILTROS METALICOS PRIMERA ETAPA, FILTROS PLISADOS MERV-10 SEGUNDA ETAPA","2021-09-20","BOS INTERNATIONAL",null,1,"5CDAHF218E825S"]
["CDAHF2-25/25","10","460/3/60",650,null,null,"SWITCH, FILTROS METALICOS PRIMERA ETAPA, FILTROS PLISADOS MERV-10 SEGUNDA ETAPA","2021-09-20","BOS INTERNATIONAL",null,6,"5CDAHF225H650S"]
["HAIT-1250-2","2","230/3/60",575,null,null,"SWITCH. MALLA EN DESCARGA","2021-09-20","BOS INTERNATIONAL",null,5,"5HAIT1250D57MA"]
["CLT-12","3/4","220/1/60",1525,null,null,"CUBREMOTOR","2021-09-27","EURO-AIRE",null,2,"5CLTG1251525CM"]
["CDAVF1-12/12","3","230/3/60",1230,null,null,null,"2021-09-27","BV EQUIPOS INDUSTRIAL",null,1,"5CDAVF112E1230"]
["CLT-16","1 1/2","220/1/60",1500,null,null,null,"2021-09-27","SERKING",null,1,"5CLTG167001500"]
["HIB-630","-","-",525,null,null,"SIN MOTOR, CON TRANSMISION ","2021-09-27","SERKING",null,3,"5HIB631SM"]
["HIB-800","-","-",570,null,null,"SIN MOTOR, CON TRANSMISION ","2021-09-27","SERKING",null,3,"5HIB801SM"]
["CDAVF2-20/20","7 1/2","208/3/60","750",null,null,"SW","2021-09-27","BOS INTERNATIONAL",null,1,"5CDAVF220G750S"]
["CCL-7/7","3/4","127/1/60","1400",null,null,null,"2021-09-29","REFRIMUNDO",null,1,"5CCL7750140000"]
["CMI-250","1/4","220/1/60","2075",null,null,"ENHUACALADO","2021-09-29","REFRIMUNDO",null,2,"5CMI2502002075"]
["C/DAHF2-18/18","1 1/2","230/3/60",500,null,null,null,"2021-10-01","VENTILACION INDUSTRIAL",null,1,"5CDAHF218C0500"]
["PORTAFILTRO WX-630","-","-","-",null,null,"BANCO PORTAFILTROS WX-630, CON BRIDAS ","2021-10-05","MOEGSA",null,2,"5PF630WX"]
["CLT-18","5","230/3/60","1775",null,null,null,"2021-10-14T11:46:20","BV EQUIPOS INDUSTRIAL",null,2,"5CLTH18F017750","5CLTG18F017750-OBSOLETO (No se puede habilitar debido a que no cumple con la clasificación actual para los CLT )"]
["CLT-22","2","230/3/60","975",null,null,null,"2021-10-15T13:48:08","BV EQUIPOS INDUSTRIAL",null,2,"5CLTG22D097500"]
["TBN-T-I-315","1","230/3/60","2300",null,null,null,"2021-10-20T10:23:12","BOS INTERNATIONAL",null,1,"5TBNTI315B2300"]
["CDAVF2-22/22","10","460/3/60","675",null,null,"PRIMERA ETAPA FILTROS MERV-8, SEGUNDA ETAPA FILTROS MERV-11, ENHUACALADO ","2021-10-25","BOS INTERNATIONAL",null,5,"5CDAVF222H0676"]
["HXP/6-800/L","3/4","460/3/60","1135",null,null,"MOTOR APEX (2-MO-75MTAPX)","2021-10-25","BOS INTERNATIONAL",null,7,"5HXP6-800/LAPX "]
["CRVL-T-16","1 1/2","127/1/60","1350",null,null,"TRAMPA DE GRASA","2021-10-26","MOVARIA",null,4,"5CRVLT167135TG"]
["CRVL-T-20","2","127/1/60","1350",null,null,"TRAMPA DE GRASA","2021-10-26","MOVARIA",null,1,"5CVRLT201135TG"]
["PF-800WX","-","-","-",null,null,"BANCO PORTAFILTROS WX-800 CON BRIDAS Y FILTROS METALICOS LAVABLES ","2021-10-27","MOEGSA",null,1,"5PF800WXFI "]
["DA-15/15","1 1/2","220/1/60","925",null,null,null,"2021-10-28","MOEGSA",null,4,"5DA15157092500"]
["DA-7/7","1 1/2","220/1/60","2075",null,null,null,"2021-10-28","MOEGSA",null,4,"5DA77720750000"]
["CMI-400","3","230/3/60","1900",null,null,"ENHUACALADO","2021-11-08","BV EQUIPOS INDUSTRIAL",null,1,"5CMI400E190000"]
["CMI-355","3","230/3/60","2475",null,null,"ENHUACALADO","2021-11-08","BV EQUIPOS INDUSTRIAL",null,1,"5CMI355E247500"]
["BDBI-280",{"$nulls":5},"ENHUACALADO","2021-11-08","S&P COLOMBIA",null,15,"5BDBI2800000CO"]
["BDBI-315",{"$nulls":5},"ENHUACALADO","2021-11-08","S&P COLOMBIA",null,5,"5BDBI3150000CO"]
["CMI-280","1/2","220/1/60","1850",null,null,"ENHUACALADO","2021-11-08","BV EQUIPOS INDUSTRIAL",null,2,"5CMI2804185100"]
["CMI-280","3/4","230/3/60","2175",null,null,"ENHUACALADO","2021-11-08","BV EQUIPOS INDUSTRIAL",null,1,"5CMI280A217600"]
["CMI-355","1/2","230/3/60","1425",null,null,"ENHUACALADO","2021-11-08","BV EQUIPOS INDUSTRIAL",null,1,"5CMI3559014260"]
["CMI-400","3","230/3/60","1900",null,null,"ENHUACALADO","2021-11-08","BV EQUIPOS INDUSTRIAL",null,1,"5CMI400E190000"]
["CMI-400","1 1/2","230/3/60","1550",null,null,"ENHUACALADO","2021-11-08","BV EQUIPOS INDUSTRIAL",null,1,"5CMI400C155000"]
["CMI-355","3","230/3/60","2475",null,null,"ENHUACALADO","2021-11-08","BV EQUIPOS INDUSTRIAL",null,1,"5CMI355E247500"]
["C/DAHF1-20/20","7 1/2","230/3/60","650",null,null,"ENHUACALADO","2021-11-08","BV EQUIPOS INDUSTRIAL",null,1,"5CDAHF120G0650"]
["C/DAHF1-20/20","1","230/3/60","425",null,null,"ENHUACALADO","2021-11-08","BV EQUIPOS INDUSTRIAL",null,1,"5CDAHF120B0425"]
["CCK-9/9","1","220/1/60","1200",null,null,"ENHUACALADO","2021-11-08","S&P PERÚ",null,1,"5CCK99601200PU"]
["CCK-9/9","3/4","220/1/60",1100,null,null,"ENHUACALADO","2021-11-08","S&P PERÚ",null,1,"5CCK99501100PU"]
["C/DAH-18/18","2","380/3/60",600,null,null,"ENHUACALADO","2021-11-08","S&P PERÚ",null,1,"5CDAH18D0600PU"]
["CRVL-T-20","2","230/3/60",1250,null,null,"TRAMPA GRASERA","2021-11-10","VENTILACION INDUSTRIAL",null,1,"5CRVLT20D125TG"]
["CRVL-T-20","1","230/3/60",1075,null,null,"TRAMPA GRASERA","2021-11-10","VENTILACION INDUSTRIAL",null,1,"5CRVLT20B107TG"]
["CRVL-T-18","2","230/3/60",1125,null,null,"TRAMPA GRASERA","2021-11-10","VENTILACION INDUSTRIAL",null,1,"5CRVLT18D112TG"]
["CRVL-T-18","1","230/3/60",1125,null,null,"TRAMPA GRASERA","2021-11-10","VENTILACION INDUSTRIAL",null,2,"5CRVLT18B112TG"]
["CRHLT-26","1 1/2","460/3/60",650,null,null,"SWITCH","2021-11-11","REFRIMUNDO",null,1,"5CRHLT26C0650S"]
["CMI-1400","25","460/3/60",525,null,null,"SWITCH","2021-11-11","REFRIMUNDO",null,2,"5CMI1400P0525S"]
["CRVHT-24","5","230/3/60",1175,null,null,"TRAMPA GRASERA","2021-11-16","SOLUCIONES EN FRIO",null,1,"5CRVHT24F117TG"]
["CMI-315","1","230/3/60",2100,null,null,"CODIGO OBSOLETO(5CMI315B021250) ENHUACALADO","2021-11-26","MOEGSA",null,8,"5CMI315B021010"]
["CMI-315","3/4","230/3/60",1850,null,null,"CODIGO OBSOLETO(5CMI315A018510) ENHUACALADO","2021-11-26","MOEGSA",null,8,"5CMI315A018510"]
["CMI-450","5","230/3/60",1950,null,null,"ENHUACALADO","2021-11-26","MOEGSA",null,4,"5CMI450F019500"]
["CMI-315","1/2","230/3/60",1650,null,null,"ENHUACALADO","2021-11-26","MOEGSA",null,8,"5CMI3159016500"]
["CMX-250/4P","1/4","230/3/60",1750,null,null,"ENHUACALADO","2021-11-26","MOEGSA",null,2,"5CMX2504801750"]
["CMI-400","5","230/3/60",2275,null,null,"ENHUACALADO","2021-11-26","MOEGSA",null,4,"5CMI400F022750"]
{"$rows_empty":1048374}
[{"$nulls":8},"S&P PERÚ"]

{"sheet":"Hoja1","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Hoja2","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}